;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 2003-2007 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;
; INF for the Intel(R) QuickData Technology device 
; (Windows Server 2003) 
;

[Version]
Signature="$Windows NT$"
Class=System
ClassGUID={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTC%
CatalogFile=qd25232.cat
DriverVer=01/18/2008,1.2.79.9

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
qd25232.sys = 1

[Manufacturer]
%MfgName% = Intel, NTx86, NTx86.5.2, NTx86.6.0
 
[Intel]
%PCI\VEN_8086&DEV_402F.DeviceDesc%=NO_DRV, PCI\VEN_8086&DEV_402F

[Intel.NTx86]
%PCI\VEN_8086&DEV_402F.DeviceDesc%=NO_DRV, PCI\VEN_8086&DEV_402F

[Intel.NTx86.5.2]
%PCI\VEN_8086&DEV_402F.DeviceDesc%=ioatdma.Dev, PCI\VEN_8086&DEV_402F

; 6.0 not supported in this INF.
[Intel.NTx86.6.0]

[DestinationDirs]
ioatdma.Files.Ext = 10,System32\Drivers

[ioatdma.Dev.NT]
CopyFiles=ioatdma.Files.Ext
AddReg=ioatdma.Driver.AddReg

[ioatdma.Dev.NT.Services]
Addservice = ioatdma, 0x00000002, ioatdma.AddService, ioatdma.EventLog

;---------------------------------------------------------------;
;-------------- Driver installation
;---------------------------------------------------------------;

[ioatdma.AddService]
DisplayName    = %ioatdma.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_BOOT_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\qd25232.sys
AddReg         = ioatdma.Service.AddReg
LoadOrderGroup = NDIS 

[ioatdma.Service.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,qd25232.sys

[ioatdma.Files.Ext]
qd25232.sys

[ioatdma.Driver.AddReg]
HKR,,Version,,"%DriverVer%"
HKR,,EnableIOAT,0x00010001, 0x00000001

;---------------------------------------------------------------;
;-------------- Event Log
;---------------------------------------------------------------;

[ioatdma.EventLog]
AddReg = ioatdma.AddEventLog.reg

[ioatdma.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%SystemRoot%\System32\ntdll.dll"
HKR, , TypesSupported,   0x00010001, 7

;---------------------------------------------------------------;
;-------------- NO_DRV installation
;---------------------------------------------------------------;

[NO_DRV]
AddReg=NoDrv.reg
Include=machine.inf
Needs=NO_DRV

[NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[NoDrv.reg]
HKR,,Version,,"%DriverVer%"

;---------------------------------------------------------------;

;-----------------------------------------------------------------------------
; Localizable Strings

[Strings]
INTC="Intel"
Disk_Description="Intel(R) QuickData Technology device"
MfgName="Intel"
PCI\VEN_8086&DEV_402F.DeviceDesc="Intel(R) 5400 Chipset QuickData Technology device - 402F"
ioatdma.SvcDesc="Intel(R) QuickData Technology device" 

;---------------------------------------------------------------------------------------------------
